WS1000 COLOR WITH 230 V DRIVE OUTPUTS:

WS1000 Color-4 control system invitation to tender

Central unit with weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver) and wireless indoor sensor WGTH-UP (for temperature and relative humidity). 4 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 4 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 4 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for Elsner Elektronik exhaust air extraction units, relays, RF relays, RF-MSG motor control unit, fan modules RF-VM, indoor sensors WG (AQS)TH-UP and WGT, key interface RF-B2-UP, Remo 8 remote control). 
Manual control for the connected drives/units via 8.4-inch real glass touch display. Connections for 10 external hand keys Remo 8 wireless remote control optional.
Central unit dimensions 250 x 182 x 43 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 235 x 169 x 62 (W x H x D in mm). Weather station dimensions 96 x 77 x 118 (W x H x D in mm). Indoor sensor housing dimensions 55 x 55 x 15 (W x H x installation depth in mm), wall mounting in junction box, with frame.
Available in white/grey or white aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1000 Color-4

WS1000 Color-6 control system invitation to tender

Central unit with weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver) and wireless indoor sensor WGTH-UP (for temperature and relative humidity). 6 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 4 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 4 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for Elsner Elektronik exhaust air extraction units, relays, RF relays, RF-MSG motor control unit, fan modules RF-VM, indoor sensors WG (AQS)TH-UP and WGT, key interface RF-B2-UP, Remo 8 remote control). 
Manual control for the connected drives/units via 8.4-inch real glass touch display. Connections for 10 external hand keys Remo 8 wireless remote control optional.
Central unit dimensions 250 x 182 x 43 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 235 x 169 x 62 (W x H x D in mm). Weather station dimensions 96 x 77 x 118 (W x H x D in mm). Indoor sensor housing dimensions 55 x 55 x 15 (W x H x installation depth in mm), wall mounting in junction box, with frame.
Available in white/grey or white aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1000 Color-6

WS1000 Color-8 control system invitation to tender

Central unit with weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver) and wireless indoor sensor WGTH-UP (for temperature and relative humidity). 8 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 4 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 4 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for Elsner Elektronik exhaust air extraction units, relays, RF relays, RF-MSG motor control unit, fan modules RF-VM, indoor sensors WG (AQS)TH-UP and WGT, key interface RF-B2-UP, Remo 8 remote control).
Manual control for the connected drives/units via 8.4-inch real glass touch display. Connections for 10 external hand keys Remo 8 wireless remote control optional.
Central unit dimensions 250 x 182 x 43 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 235 x 169 x 62 (W x H x D in mm). Weather station dimensions 96 x 77 x 118 (W x H x D in mm). Indoor sensor housing dimensions 55 x 55 x 15 (W x H x installation depth in mm), wall mounting in junction box, with frame.
Available in white/grey or white aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1000 Color-8

WS1000 Color-10 control system invitation to tender

Central unit with weather station (with wind sensor, heated rain sensor, brightness sensor, temperature sensor, GPS receiver) and wireless indoor sensor WGTH-UP (for temperature and relative humidity). 10 drive output 230 V (for blinds, shutters, roller shutters, windows, sliding door), 4 multi-function outputs (for heating, cooling, ventilation unit, alarm, roof gutter heating, lighting, dimmer). 4 multi-function inputs (for motion detectors, smoke alarms, closed contact, status message for a separate air conditioning system, automatic functions reset). 32 free wireless channels (for Elsner Elektronik exhaust air extraction units, relays, RF relays, RF-MSG motor control unit, fan modules RF-VM, indoor sensors WG (AQS)TH-UP and WGT, key interface RF-B2-UP, Remo 8 remote control). 
Manual control for the connected drives/units via 8.4-inch real glass touch display. Connections for 10 external hand keys Remo 8 wireless remote control optional.
Central unit dimensions 250 x 182 x 43 (W x H x installation depth in mm), flush or cavity wall mounting, dimensions of flush mounting box 235 x 169 x 62 (W x H x D in mm). Weather station dimensions 96 x 77 x 118 (W x H x D in mm). Indoor sensor housing dimensions 55 x 55 x 15 (W x H x installation depth in mm), wall mounting in junction box, with frame.
Available in white/grey or white aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: WS1000 Color-10

REMOTE CONTROL FOR WS1000 COLOR:

Remo 8 wireless remote control invitation to tender

Hand-held transmitter with 8 channels. Up/Down/Stop keys, display for channel indication. With magnetic wall bracket.
Hand-held transmitter dimensions 41 x 140 x 21 (W x H x D in mm). Wall bracket dimensions 54 x 150 x 11 (W x H x D in mm).
Available in white/grey or aluminium/graphite.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: Remo 8