KNX PS640 power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640

KNX PS640 USB power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset. Front panel USB socket for bus access.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640 USB

KNX PS640+ power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset. Bus functions: Transfer of fault reports and operating data, time/duration reset.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640+

KNX PS640+USB power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset. Bus functions: Transfer of fault reports and operating data, time/duration reset. Front panel USB socket for bus access.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640+USB

KNX PS640-IP power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset. Ethernet interface for routing, tunnelling and for Ethernet as line coupler and range coupler.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640-IP	

KNX PS640+IP power supply invitation to tender

Power supply for the KNX bus system. One output KNX bus voltage 29 V (throttled), max. output current 640 mA, short circuit-proof. One output 24 V DC (no throttle), max. output current 150 mA. Functions on the device (via integrated display and keypad): Logging of fault reports, indication of bus voltage and bus current, reset. Bus functions: Transfer of fault reports and operating data, time/duration reset. Ethernet interface for routing, tunnelling and for Ethernet as line coupler and range coupler.
Rail-mounted device for busbar mounting. Dimensions 123 x 89 x 61 (W x H x D in mm), 7 Units.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX PS640+IP