KNX Touch One invitation to tender 

Touch panel for room automation with KNX, with integrated control functions. Colour touch display (5.7 inches) for operation and automatic function setting. Internal automatic functions for shading (sun-/eye protection), for ambient climate control (heating, cooling, exhaust air extraction) and for lighting control. Default setting via ETS. Bus functions for time and scene control. Freely configurable display and control elements on the display.
Integrated indoor sensor for temperature and air humidity. 4 binary inputs. KNX connection for data transfer. Remo 8 wireless remote control optional.

Operating voltage: 12 to 40 V DC. Dimensions approx. 164 x 121 x 29 (W x H x D, mm) Surface mounting via an equipment socket. Colour: white/grey.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: KNX Touch One