Tender specifications Weather station P04i-GPS

Weather station for direct connection to KNX WS1000 Colour/Style, WS1000 Colour/Style and WS1 Colour/Style controllers. Recording of brightness, wind speed (electronic sensor), precipitation (heated sensor) and temperature. With GPS receiver. Including bracket for wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm). Optional connection via P03i/P04i data logger or P03i/P04i distributor.

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: P04i-GPS

Tender specifications Wind sensor P04i-W

Wind sensor for KNX WS1000 Colour/Style, WS1000 Colour/Style and WS1 Colour/Style controllers. Connection via P03i/Po04i data logger. Detection of wind speed (electronic measurement). Including bracket for wall/mast mounting. Dimensions 62 x 71 x 145 (W x H x D in mm).

Manufactured by: Elsner Elektronik (www.elsner-elektronik.de)
Type: P04i-W